For 1990-2009 cars

# Car Care Matrix for Warranty Administration

Subject: | Car Care Matrix for Warranty Administration

Models: | 2005 Model Year Saturn Vehicles

Attention: | Fixed Operations Manager and Technician

This bulletin is being updated to delete the timing belt replacement and transfer assembly fluid replacement from 25,000 mile service. Please discard Corporate Bulletin Number 05-00-90-002 (Section 00 - General Information).

Important: This service bulletin is not applicable to Saturn retailers in Canada.

The purpose of this bulletin is to provide Saturn retailers with new warranty administration information.

2005 AWD VUE SCHEDULED MAINTENANCE
MAINTENANCE INTERVAL | SERVICE | LABOR OP | LABOR TIME
MAINT. I | - Change engine oil filter. | X3600 | 0.9
| - Visually check for any leaks or damages. Note: Have the system inspected and repaired and the fluid level checked. Add fluid if needed. |  |
| - Rotate tires and check inflation pressures and wear. |  |
| - Inspect brake system. Note: Visually inspect brake lines and hoses for proper hook-up, binding, leaks, cracks, chafing, etc. Inspect disc brake pads for wear and rotors for surface condition. Inspect drum brake linings for wear or cracks. Inspect other brake parts, including drums, wheel cylinders, calipers, parking brake, etc. |  |
| - Check engine coolant and windshield washer fluid levels and add fluid as needed. |  |
MAINT. II | Services Provided for Maintenance I Plus: | X3610 | 1.2
| - Inspect engine air cleaner filter. If necessary, replace filter. Note: If car is driven under dusty conditions regularly, inspect the filter at each engine oil change. |  |
| - Inspect suspension and steering components. Note: Visually inspect front and rear suspension and steering system for damaged, loose, or missing parts or signs of wear. |  |
| - Inspect engine cooling system. Note: Visually inspect hoses and have them replaced if they are cracked, swollen, or deteriorated. Inspect all pipes, fittings, and clamps; replace with genuine Saturn parts as needed. A pressure test of the cooling system and pressure cap and cleaning the outside of the radiator and air conditioning condenser is recommended at least once a year. |  |
| - Inspect wiper blades. Note: Visually inspect wiper blades for wear or cracking. Replace blade inserts that appear worn or damaged or that streak or miss areas of the windshield. |  |
| - Inspect restraint system components. Note: Verify safety belt reminder light and all belts, buckles, latch plates, retractors, and anchorages are working properly. Have safety belt repaired if needed. Replace any torn or frayed safety belts. Repair or replace any open any opened or broken airbag coverings. |  |
| - Lubricate body components. Note: Lubricate all key lock cylinders, door hinges and latches, hood hinges and latches, glove box hinges, sunroof (if equipped), and any folding seat hardware. More frequent lubrication may be required when exposed to a corrosive environment. Applying silicone grease on weather-strips with a clean cloth will make them last longer, seal better, and not stick or squeak. |  |
| - Replace passenger compartment air filter. Note: Or every 12 months, whichever comes first. If car is driven under dusty conditions regularly, the filter may require replacement more often. |  |
| - L4 Engine: Inspect throttle system. Note: Check system for interference or binding and for damaged or missing parts. Replace parts as needed. Replace any components that have high effort or excessive wear. |  |
25,000 MILES | Maintenance I Plus: Additional Requirements | X3620 (AUTO) | 1
| - Inspect fuel system for damage or leaks. |  |
| - Inspect exhaust system for loose or damaged components. |  |
| - V6 Engine: Change automatic transaxle fluid (severe service). Note: Severe service is when vehicle is mainly driven under one or more of the following conditions:

• | In the heavy traffic where the outside temperature regularly reaches 90°F (32°C) or higher

• | In hilly or mountainous terrain

• | When doing frequent trailer towing

0.3

| - Inspect engine accessory belt. |  |
25,000 MILES | Maintenance I Plus: Additional Requirements | X3620 (MANUAL) | 1
| - Inspect fuel system for damage or leaks. |  |
| - Inspect exhaust system for loose or damaged components. |  |
25,000 MILES | Maintenance II Plus: Additional Requirements | X3620 (AUTO) | 1.3
| - Inspect fuel system for damage or leaks. |  |
| - Inspect exhaust system for loose or damaged components. |  |
| - V6 Engine: Change automatic transaxle fluid (severe service). Note: Severe service is when vehicle is mainly driven under one or more of the following conditions:

• | In the heavy traffic where the outside temperature regularly reaches 90°F (32°C) or higher

• | In hilly or mountainous terrain

• | When doing frequent trailer towing

0.3

| - V6 Engine: Change transfer assembly fluid (severe service). Note: Severe service is when vehicle is mainly driven under one or more of the following conditions:

• | In the heavy traffic where the outside temperature regularly reaches 90°F (32°C) or higher

• | In hilly or mountainous terrain

• | When doing frequent trailer towing

0.2

| - Inspect engine accessory belt. |  |
25,000 MILES | Maintenance II Plus: Additional Requirements | X3620 (MANUAL) | 1.3
| - Inspect fuel system for damage or leaks. |  |
| - Inspect exhaust system for loose or damaged components. |  |
| - Inspect engine accessory belt. |  |
50,000 MILES | Maintenance I Plus: Additional Requirements | X3630 (AUTO) | 1
| - Inspect fuel system for damage or leaks. |  |
| - Inspect exhaust system for loose or damaged components. |  |
| - Inspect engine accessory belt. |  |
| - Replace engine air cleaner filter. |  |
| - VTi variable transaxle: Add DEX-CVT additive |  | 0.1
| - L4 engine: Change VTi variable transaxle fluid (severe service). Note: Severe service is when vehicle is mainly driven under one or more of the following conditions:

• | In the heavy traffic where the outside temperature regularly reaches 90°F (32°C) or higher

• | In hilly or mountainous terrain

• | When doing frequent trailer towing

0.4

| - V6 Engine: Replace timing belt (severe service). Note: Severe service is when vehicle is mainly driven under one or more of the following conditions:

• | In very high temperatures -- over 110°F (43°C)

• | In very low temperatures -- under -29°F (-29°C)

• | When doing frequent trailer towing

2.2

| - V6 Engine: Change automatic transaxle fluid (severe service). Note: Severe service is when vehicle is mainly driven under one or more of the following conditions:

• | In the heavy traffic where the outside temperature regularly reaches 90°F (32°C) or higher

• | In hilly or mountainous terrain

• | When doing frequent trailer towing

0.3

| - L4 Engine: Change rear drive module power takeoff unit fluid (severe service). Note: Severe service is when vehicle is mainly driven under one or more of the following conditions:

• | In the heavy traffic where the outside temperature regularly reaches 90°F (32°C) or higher

• | In hilly or mountainous terrain

• | When doing frequent trailer towing

0.3

| - V6 Engine: Change transfer assembly fluid (severe service). Note: Severe service is when vehicle is mainly driven under one or more of the following conditions:

• | In the heavy traffic where the outside temperature regularly reaches 90°F (32°C) or higher

• | In hilly or mountainous terrain

• | When doing frequent trailer towing

0.2

| - V6 Engine: Change rear drive module fluid (severe service). Note: Severe service is when vehicle is mainly driven under one or more of the following conditions:

• | In the heavy traffic where the outside temperature regularly reaches 90°F (32°C) or higher

• | In hilly or mountainous terrain

• | When doing frequent trailer towing

0.3

50,000 MILES | Maintenance I Plus: Additional Requirements | X3630 (MANUAL) | 1
| - Inspect fuel system for damage or leaks. |  |
| - Inspect exhaust system for loose or damaged components. |  |
| - Inspect engine accessory belt. |  |
| - Replace engine air cleaner filter. |  |
50,000 MILES | Maintenance II Plus: Additional Requirements | X3630 (AUTO) | 1.3
| - Inspect fuel system for damage or leaks. |  |
| - Inspect exhaust system for loose or damaged components. |  |
| - Inspect engine accessory belt. |  |
| - Replace engine air cleaner filter. |  |
| - VTi variable transaxle: Add DEX-CVT additive. Note: Severe service is when vehicle is mainly driven under one or more of the following conditions:

• | In very high temperatures -- over 110°F (43°C)

• | In very low temperatures -- under -29°F (-29°C)

• | When doing frequent trailer towing

0.4

| - V6 Engine: Replace timing belt (severe service). Note: Severe service is when vehicle is mainly driven under one or more of the following conditions:

• | In very high temperatures -- over 110°F (43°C)

• | In very low temperatures -- under -29°F (-29°C)

• | When doing frequent trailer towing

2.2

| - V6 Engine: Change automatic transaxle fluid (severe service). Note: Severe service is when vehicle is mainly driven under one or more of the following conditions:

• | In the heavy traffic where the outside temperature regularly reaches 90°F (32°C) or higher

• | In hilly or mountainous terrain

• | When doing frequent trailer towing

0.3

| - L4 Engine: Change rear drive module power takeoff unit fluid (severe service). Note: Severe service is when vehicle is mainly driven under one or more of the following conditions:

• | In the heavy traffic where the outside temperature regularly reaches 90°F (32°C) or higher

• | In hilly or mountainous terrain

• | When doing frequent trailer towing

0.3

| - V6 Engine: Change transfer assembly fluid (severe service). Note: Severe service is when vehicle is mainly driven under one or more of the following conditions:

• | In the heavy traffic where the outside temperature regularly reaches 90°F (32°C) or higher

• | In hilly or mountainous terrain

• | When doing frequent trailer towing

0.2

| - V6 Engine: Change rear drive module fluid (severe service). Note: Severe service is when vehicle is mainly driven under one or more of the following conditions:

• | In the heavy traffic where the outside temperature regularly reaches 90°F (32°C) or higher

• | In hilly or mountainous terrain

• | When doing frequent trailer towing

0.3

50,000 MILES | Maintenance II Plus: Additional Requirements | X3630 (MANUAL) | 1.3
| - Inspect fuel system for damage or leaks. |  |
| - Inspect exhaust system for loose or damaged components. |  |
| - Inspect engine accessory belt. |  |
| - Replace engine air cleaner filter. |  |

2005 FWD VUE SCHEDULED MAINTENANCE
MAINTENANCE INTERVAL | SERVICE | LABOR OP | LABOR TIME
MAINT. I | - Change engine oil. | X3600 | 0.9
| - Visually check for any leaks or damages. Note: Have the system inspected and repaired and the fluid level checked. Add fluid if needed. |  |
| - Rotate tires and check inflation pressures and wear. |  |
| - Inspect brake system. Note: Visually inspect brake lines and hoses for proper hook-up, binding, leaks, cracks, chafing, etc. Inspect disc brake pads for wear and rotors for surface condition. Inspect drum brake linings for wear or cracks. Inspect other brake parts, including drums, wheel cylinders, calipers, parking brake, etc. |  |
| - Check engine coolant and windshield washer fluid levels and add fluid as needed. |  |
MAINT. II | Services Provided for Maintenance I Plus: | X3610 | 1.2
| - Inspect engine air cleaner filter. If necessary, replace filter. Note: If car is driven under dusty conditions regularly, inspect the filter at each engine oil change. |  |
| - Inspect suspension and steering components. Note: Visually inspect front and rear suspension and steering system for damaged, loose, or missing parts or signs of wear. |  |
| - Inspect engine cooling system. Note: Visually inspect hoses and have them replaced if they are cracked, swollen, or deteriorated. Inspect all pipes, fittings, and clamps; replace with genuine Saturn parts as needed. A pressure test of the cooling system and pressure cap and cleaning the outside of the radiator and air conditioning condenser is recommended at least once a year. |  |
| - Inspect wiper blades. Note: Visually inspect wiper blades for wear or cracking. Replace blade inserts that appear worn or damaged or that streak or miss areas of the windshield. |  |
| - Inspect restraint system components. Note: Verify safety belt reminder light and all belts, buckles, latch plates, retractors, and anchorages are working properly. Have safety belt repaired if needed. Replace any torn or frayed safety belts. Repair or replace any open any opened or broken airbag coverings. |  |
| - Lubricate body components. Note: Lubricate all key lock cylinders, door hinges and latches, hood hinges and latches, glove box hinges, sunroof (if equipped), and any folding seat hardware. More frequent lubrication may be required when exposed to a corrosive environment. Applying silicone grease on weather-strips with a clean cloth will make them last longer, seal better, and not stick or squeak. |  |
| - Replace passenger compartment air filter. Note: Or every 12 months, whichever comes first. If car is driven under dusty conditions regularly, the filter may require replacement more often. |  |
| - L4 Engine: Inspect throttle system. Note: Check system for interference or binding and for damaged or missing parts. Replace parts as needed. Replace any components that have high effort or excessive wear. |  |
25,000 MILES | Maintenance I Plus: Additional Requirements | X3620 (AUTO) | 1
| - Inspect fuel system for damage or leaks. |  |
| - Inspect exhaust system for loose or damaged components. |  |
| - V6 Engine: Change automatic transaxle fluid (severe service). Note: Severe service is when vehicle is mainly driven under one or more of the following conditions:

• | In the heavy traffic where the outside temperature regularly reaches 90°F (32°C) or higher

• | In hilly or mountainous terrain

• | When doing frequent trailer towing

0.3

25,000 MILES | Maintenance II Plus: Additional Requirements | X3620 (AUTO) | 1.3
| - Inspect fuel system for damage or leaks. |  |
| - Inspect exhaust system for loose or damaged components. |  |
| - V6 Engine: Change automatic transaxle fluid (severe service). Note: Severe service is when vehicle is mainly driven under one or more of the following conditions:

• | In the heavy traffic where the outside temperature regularly reaches 90°F (32°C) or higher

• | In hilly or mountainous terrain

• | When doing frequent trailer towing

0.3

25,000 MILES | Maintenance II Plus: Additional Requirements | X3620 (MANUAL) | 1.3
| - Inspect fuel system for damage or leaks. |  |
| - Inspect exhaust system for loose or damaged components. Note: Severe service is when vehicle is mainly driven under one or more of the following conditions:

• | In the heavy traffic where the outside temperature regularly reaches 90°F (32°C) or higher

• | In hilly or mountainous terrain

• | When doing frequent trailer towing

50,000 MILES | Maintenance I Plus: Additional Requirements | X3630 (AUTO) | 1
| - Inspect fuel system for damage or leaks. |  |
| - Inspect exhaust system for loose or damaged components. |  |
| - Inspect engine accessory belt. |  |
| - Replace engine air cleaner filter. |  |
| - L4 engine: Change auto trans fluid (severe service). Note: Severe service is when vehicle is mainly driven under one or more of the following conditions:

• | In very high temperatures -- over 110°F (43°C)

• | In very low temperatures -- under -29°F (-29°C)

• | When doing frequent trailer towing

0.3

| - V6 Engine: Change automatic transaxle fluid (severe service). Note: Severe service is when vehicle is mainly driven under one or more of the following conditions:

• | In the heavy traffic where the outside temperature regularly reaches 90°F (32°C) or higher

• | In hilly or mountainous terrain

• | When doing frequent trailer towing

0.3

50,000 MILES | Maintenance I Plus: Additional Requirements | X3630 (MANUAL) | 1
| - Inspect fuel system for damage or leaks. |  |
| - Inspect exhaust system for loose or damaged components. |  |
| - Inspect engine accessory belt. |  |
| - Replace engine air cleaner filter. |  |
50,000 MILES | Maintenance II Plus: Additional Requirements | X3630 (AUTO) | 1.3
| - Inspect fuel system for damage or leaks. |  |
| - Inspect exhaust system for loose or damaged components. |  |
| - Inspect engine accessory belt. |  |
| - Replace engine air cleaner filter. |  |
| - Replace timing belt. |  |
| - L4 engine: Change auto trans fluid (severe service). Note: Severe service is when vehicle is mainly driven under one or more of the following conditions:

• | In very high temperatures -- over 110°F (43°C)

• | In very low temperatures -- under -29°F (-29°C)

• | When doing frequent trailer towing

0.3

| - V6 Engine: Change automatic transaxle fluid (severe service). Note: Severe service is when vehicle is mainly driven under one or more of the following conditions:

• | In the heavy traffic where the outside temperature regularly reaches 90°F (32°C) or higher

• | In hilly or mountainous terrain

• | When doing frequent trailer towing

0.3

50,000 MILES | Maintenance II Plus: Additional Requirements | X3630 (MANUAL) | 1.3
| - Inspect fuel system for damage or leaks. |  |
| - Inspect exhaust system for loose or damaged components. |  |
| - Inspect engine accessory belt. |  |
| - Replace engine air cleaner filter. |  |

2005 Relay SCHEDULED MAINTENANCE
MAINTENANCE INTERVAL | SERVICE | LABOR OP | LABOR TIME
MAINT. I | - Change engine oil filter. | X3600 | 0.9
| - Lubricate chassis components. |  |
| - Visually check for any leaks or damages. Note: Have the system inspected and repaired and the fluid level checked. Add fluid if needed. |  |
| - Inspect engine air cleaner filter. If necessary, replace filter. Note: If car is driven under dusty conditions regularly, inspect the filter at each engine oil change. |  |
| - Rotate tires and check inflation pressures and wear. |  |
| - Inspect brake system. Note: Visually inspect brake lines and hoses for proper hook-up, binding, leaks, cracks, chafing, etc. Inspect disc brake pads for wear and rotors for surface condition. Inspect other brake parts, including drums, wheel cylinders, calipers, parking brake, etc. |  |
MAINT. II | Services Provided for Maintenance I Plus: | X3610 | 1.2
| - Inspect suspension and steering components. Note: Visually inspect front and rear suspension and steering system for damaged, loose, or missing parts or signs of wear or lack of lubrication. Inspect power steering lines and hoses for proper hook-up, bindings, leaks, cracks, chafing, etc. |  |
| - Inspect engine cooling system. Note: Visually inspect hoses and have them replaced if they are cracked, swollen, or deteriorated. Inspect all pipes, fittings, and clamps; replace with genuine Saturn parts as needed. A pressure test of the cooling system and pressure cap and cleaning the outside of the radiator and air conditioning condenser is recommended at least once a year. |  |
| - Inspect wiper blades. Note: Visually inspect wiper blades for wear or cracking. Replace blade inserts that appear worn or damaged or that streak or miss areas of the windshield. |  |
| - Inspect restraint system components. Note: Verify safety belt reminder light and all belts, buckles, latch plates, retractors, and anchorages are working properly. Have safety belt repaired if needed. Replace any torn or frayed safety belts. Repair or replace any open any opened or broken airbag coverings. |  |
| - Lubricate body components. Note: Lubricate all key lock cylinders, hood latch assemblies, secondary latches, pivots, spring anchor and release pawl, hood and door hinges, rear folding seats, liftgate hinges, fuel door hinge, power sliding door cable, and sliding door track(s). More frequent lubrication may be required when exposed to a corrosive environment. Applying silicone grease on weather-strips with a clean cloth will make them last longer, seal better, and not stick or squeak. |  |
| - Check transaxle fluid level and add fluid as needed. |  |
| - Inspect throttle system. Note: Check system for interference or binding and for damaged or missing parts. Replace parts as needed. Replace any components that have high effort or excessive wear. Do not lubricate accelerator or cruise control cables. |  |
25,000 Miles | Maintenance I Plus: Additional Requirements | X3620 | 1
| - Inspect fuel system for damage or leaks. |  |
| - Inspect exhaust system for loose or damaged components. |  |
25,000 Miles | Maintenance II Plus: Additional Requirements | X3620 | 1.3
| - Inspect fuel system for damage or leaks. |  |
| - Inspect exhaust system for loose or damaged components. |  |
50,000 Miles | Maintenance I Plus: Additional Requirements | X3630 | 1
| - Inspect fuel system for damage or leaks. |  |
| - Inspect exhaust system for loose or damaged components. |  |
| - Replace engine air cleaner filter. |  |
| - Change automatic transaxle fluid and filter (severe service). Note: Severe service is when vehicle is mainly driven under one or more of the following conditions:

• | In the heavy traffic where the outside temperature regularly reaches 90°F (32°C) or higher

• | In hilly or mountainous terrain

• | When doing frequent trailer towing

0.8

50,000 Miles | Maintenance II Plus: Additional Requirements | X3630 | 1.3
| - Inspect fuel system for damage or leaks. |  |
| - Inspect exhaust system for loose or damaged components. |  |
| - Replace engine air cleaner filter. |  |
| - Change automatic transaxle fluid and filter (severe service). Note: Severe service is when vehicle is mainly driven under one or more of the following conditions:

• | In the heavy traffic where the outside temperature regularly reaches 90°F (32°C) or higher

• | In hilly or mountainous terrain

• | When doing frequent trailer towing

0.8

2005 ION SCHEDULED MAINTENANCE
MAINTENANCE INTERVAL | SERVICE | LABOR OP | LABOR TIME
MAINT. I | - Change engine oil filter. | X3600 | 0.9
| - Visually check for any leaks or damages. Note: Have the system inspected and repaired and the fluid level checked. Add fluid if needed. |  |
| - Rotate tires and check inflation pressures and wear. |  |
| - Inspect brake system. Note: Visually inspect brake lines and hoses for proper hook-up, binding, leaks, cracks, chafing, etc. Inspect disc brake pads for wear and rotors for surface condition. Inspect drum brake linings for wear or cracks. Inspect other brake parts, including drums, wheel cylinders, calipers, parking brake, etc. |  |
| - Check engine coolant and windshield washer fluid levels and add fluid as needed. |  |
MAINT. II | Services Provided for Maintenance I Plus: | X3610 | 1.2
| - Inspect engine air cleaner filter. If necessary, replace filter. Note: If car is driven under dusty conditions regularly, inspect the filter at each engine oil change. |  |
| - Replace engine air cleaner filter. |  |
| - Inspect engine accessory drive belt. |  |
| - Inspect suspension and steering components. Note: Visually inspect front and rear suspension and steering system for damaged, loose, or missing parts or signs of wear. |  |
| - Inspect engine cooling system. Note: Visually inspect hoses and have them replaced if they are cracked, swollen, or deteriorated. Inspect all pipes, fittings, and clamps; replace with genuine Saturn parts as needed. A pressure test of the cooling system and pressure cap and cleaning the outside of the radiator and air conditioning condenser is recommended at least once a year. |  |
| - Inspect wiper blades. Note: Visually inspect wiper blades for wear or cracking. Replace blade inserts that appear worn or damaged or that streak or miss areas of the windshield. |  |
| - Inspect restraint system components. Note: Verify belts, buckles, latch plates, retractors, and anchorages are working properly. Have safety belt repaired if needed. Replace any torn or frayed safety belts. Repair or replace any open any opened or broken airbag coverings. |  |
| - Lubricate body components. Note: Lubricate all key lock cylinders, door hinges and latches, hood hinges and latches, glove box hinges, sunroof (if equipped), and any folding seat hardware. More frequent lubrication may be required when exposed to a corrosive environment. Applying silicone grease on weather-strips with a clean cloth will make them last longer, seal better, and not stick or squeak. |  |
| - Replace passenger compartment air filter. Note: Or every 12 months, whichever comes first. If car is driven under dusty conditions regularly, the filter may require replacement more often. |  |
| - Inspect throttle system. Note: Check system for interference or binding and for damaged or missing parts. Replace parts as needed. Replace any components that have high effort or excessive wear. Do not lubricate accelerator or cruise control cables. |  |
25,000 Miles | Maintenance I Plus: Additional Requirements | X3620 | 1.0
| - Inspect fuel system for damage or leaks. |  |
| - Inspect exhaust system for loose or damaged components. |  |
| - Inspect engine accessory drive belt. |  |
25,000 Miles | Maintenance II Plus: Additional Requirements | X3620 | 1.3
| - Inspect fuel system for damage or leaks. |  |
| - Inspect exhaust system for loose or damaged components. |  |
| - Inspect engine accessory drive belt. |  |
50,000 Miles | Maintenance I Plus: Additional Requirements | X3630 (AUTO) | 1.0
| - Inspect fuel system for damage or leaks. |  |
| - Inspect exhaust system for loose or damaged components. |  |
| - Inspect engine accessory drive belt. |  |
| - Replace engine air cleaner filter. |  |
| - Change automatic transaxle fluid (severe service). Note: Severe service is when vehicle is mainly driven under one or more of the following conditions:

• | In the heavy traffic where the outside temperature regularly reaches 90°F (32°C) or higher

• | In hilly or mountainous terrain

• | When doing frequent trailer towing

.3

50,000 Miles | Maintenance I Plus: Additional Requirements | X3630 (Manual) | 1
| - Inspect fuel system for damage or leaks. |  |
| - Inspect exhaust system for loose or damaged components. |  |
| - Inspect engine accessory drive belt. |  |
| - Replace engine air cleaner filter. |  |
| Red Line Only: - Inspect engine accessory drive belt. |  | .2 Red Line
50,000 Miles | Maintenance II Plus: Additional Requirements | X3630 (AUTO) | 1.3
| - Inspect fuel system for damage or leaks. |  |
| - Inspect exhaust system for loose or damaged components. |  |
| - Inspect engine accessory drive belt. |  |
| - Replace engine air cleaner filter. |  |
| **Change automatic transaxle fluid (severe service). Note: Severe service is when vehicle is mainly driven under one or more of the following conditions:

• | In the heavy traffic where the outside temperature regularly reaches 90°F (32°C) or higher

• | In hilly or mountainous terrain

• | When doing frequent trailer towing

.3

50,000 Miles | Maintenance II Plus: Additional Requirements | X3630 (MANUAL) | 1
| - Inspect fuel system for damage or leaks. |  |
| - Inspect exhaust system for loose or damaged components. |  |
| - Inspect engine accessory drive belt. |  |
| - Replace engine air cleaner filter. |  |
| Red Line Only: - Inspect engine accessory drive belt. |  | .2 Red Line

2005 L300/LW300 SCHEDULED MAINTENANCE
MAINTENANCE INTERVAL | SERVICE | LABOR OP | LABOR TIME
MAINT. I | - Change engine oil filter. | X3600 | 0.9
| - Visually check for any leaks or damages. Note: Have the system inspected and repaired and the fluid level checked. Add fluid if needed. |  |
| - Rotate tires and check inflation pressures and wear. |  |
| - Inspect brake system. Note: Visually inspect brake lines and hoses for proper hook-up, binding, leaks, cracks, chafing, etc. Inspect disc brake pads for wear and rotors for surface condition. Inspect drum brake linings for wear or cracks. Inspect other brake parts, including drums, wheel cylinders, calipers, parking brake, etc. |  |
| - Check engine coolant and windshield washer fluid levels and add fluid as needed. |  |
MAINT. II | Services Provided for Maintenance I Plus: | X 3610 | 1.2
| - Inspect engine air cleaner filter. If necessary, replace filter. Note: If car is driven under dusty conditions regularly, inspect the filter at each engine oil change. |  |
| - Inspect suspension and steering components. Note: Visually inspect front and rear suspension and steering system for damaged, loose, or missing parts or signs of wear. Inspect power steering lines and hoses for proper hook-up, binding, leaks, cracks, chafing, etc. |  |
| - Inspect engine cooling system. Note: Visually inspect hoses and have them replaced if they are cracked, swollen, or deteriorated. Inspect all pipes, fittings, and clamps; replace with genuine Saturn parts as needed. A pressure test of the cooling system and pressure cap and cleaning the outside of the radiator and air conditioning condenser is recommended at least once a year. |  |
| - Inspect wiper blades. Note: Visually inspect wiper blades for wear or cracking. Replace blade inserts that appear worn or damaged or that streak or miss areas of the windshield. |  |
| - Inspect restraint system components. Note: Verify safety belt reminder light and all belts, buckles, latch plates, retractors, and anchorages are working properly. Have safety belt repaired if needed. Replace any torn or frayed safety belts. Repair or replace any open any opened or broken airbag coverings. The airbag system does not need regular maintenance. |  |
| - Lubricate body components. Note: Lubricate all key lock cylinders, door hinges and latches, hood hinges and latches, glove box hinges, sunroof (if equipped), and any folding seat hardware. More frequent lubrication may be required when exposed to a corrosive environment. Applying silicone grease on weather-strips with a clean cloth will make them last longer, seal better, and not stick or squeak. |  |
| - Replace passenger compartment air filter. Note: Or every 12 months, whichever comes first. If car is driven under dusty conditions regularly, the filter may require replacement more often. |  |
| - Inspect throttle system. Note: Check system for interference or binding and for damaged or missing parts. Replace parts as needed. Replace any components that have high effort or excessive wear. Do not lubricate accelerate or cruise control cables. |  |
25,000 MILES | Maintenance I Plus: Additional Requirements | X3620 | 1
| - Inspect fuel system for damage or leaks. |  |
| - Inspect exhaust system for loose or damaged components. |  |
| - Inspect engine accessory belt. |  |
25,000 MILES | Maintenance II Plus: Additional Requirements | X3620 | 1.3
| - Inspect fuel system for damage or leaks. |  |
| - Inspect exhaust system for loose or damaged components. |  |
| - Inspect engine accessory belt. |  |
50,000 MILES | Maintenance I Plus: Additional Requirements | X3630 (AUTO) | 1
| - Inspect fuel system for damage or leaks. |  |
| - Inspect exhaust system for loose or damaged components. |  |
| - Replace engine air cleaner filter. |  |
| - Change automatic transaxle fluid and filter (severe service). Note: Severe service is when vehicle is mainly driven under one or more of the following conditions:

• | In the heavy traffic where the outside temperature regularly reaches 90°F (32°C) or higher

• | In hilly or mountainous terrain

• | When doing frequent trailer towing

0.5

50,000 MILES | Maintenance II Plus: Additional Requirements | X3630 (AUTO) | 1.3
| - Inspect fuel system for damage or leaks. |  |
| - Inspect exhaust system for loose or damaged components. |  |
| - Replace engine air cleaner filter. |  |
| - Change automatic transaxle fluid and filter (severe service). Note: Severe service is when vehicle is mainly driven under one or more of the following conditions:

• | In the heavy traffic where the outside temperature regularly reaches 90°F (32°C) or higher

• | In hilly or mountainous terrain

• | When doing frequent trailer towing

0.5