For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the rear stabilizer bar to support assembly clamp bolts.
3. Remove the stabilizer bar clamps from the stabilizer bar.
4. Remove the insulators from the stabilizer bar.

### Installation Procedure

1. Install the insulators to the stabilizer bar.
2. Install the stabilizer bar clamps to the stabilizer bar.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the stabilizer bar clamp to support assembly bolts.

Tighten
Tighten the bolts to 55 N·m (41 lb ft).

4. Lower the vehicle.