For 1990-2009 cars

### Removal Procedure

1. Disconnect the ambient air temperature sensor electrical connector.
2. Remove the ambient air temperature sensor screw.
3. Remove the ambient air temperature sensor.

### Installation Procedure

1. Install the ambient air temperature sensor.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the screw to the ambient air temperature sensor.

Tighten
Tighten the screw to 4 N·m (35 lb in).

3. Connect the ambient air temperature sensor electrical connector.