For 1990-2009 cars

#### Tools Required

• | J 6133-A Bearing Race Installer

• | J 22828 Input/Countershaft Race Installer

1. If removed, install the 5th counter gear (3) on the countershaft (4), using a hydraulic press and J 22828 .
2. Using a hydraulic press and J 6133-A , install the countershaft rear bearing (2) onto the countershaft.
3. Install the retaining ring (1) for the countershaft rear bearing on to the countershaft.