For 1990-2009 cars

### Removal Procedure

1. Open both the front and rear doors.
2. Remove the center pillar weatherstrip using the retainer remover to release the push-in retainers.
3. Remove the weatherstrip from the center pillar.

### Installation Procedure

1. Position the center pillar weatherstrip push-in retainers to the holes in the center pillar.
2. Install the center pillar weatherstrip pressing in the retainers until fully seated.
3. Close the doors and inspect the weatherstrip for a proper fit.