For 1990-2009 cars

The M86 Getrag is a 5 speed manual transmission assembly.

Important: Use only DEXRON®III Automatic Transmission Lubricant for this manual transmission assembly. Other lubricants or additives may affect the shift performance.

The M86 Getrag manual transmission has the following features:

• | First and second gear double coned synchronizer

• | Third, fourth, and fifth gear single coned synchronizer

• | Reverse synchronized

• | Three shaft design consisting of an input shaft, output shaft, and intermediate shaft

• | Reverse inhibit feature

• | One piece clutch actuator - no bleed screw

• | Transmission venting system is part of the fill cap

• | First gear ratio is 3.58

• | Second gear ratio is 2.02

• | Third gear ratio is 1.35

• | Fourth gear ratio is 0.98

• | Fifth gear ratio is 0.69

• | Reverse gear ratio is 3.31

• | Final drive ratio is 3.94

• | Vehicle speed sensor (VSS)

The manual transmission shift cables must be adjusted for proper shifter performance.