For 1990-2009 cars

#### Tools Required

J 36850 TRANSJEL™

1. Install the final drive carrier to case thrust bearing (117) onto the final drive carrier. Retain the bearing with J 36850 .
2. Install the complete final drive carrier assembly (116) into the transmission case (51).
3. Install the thrust bearing (700) into the final drive carrier assembly (116). Retain the bearing with J 36850 .

Important: Install the sun gear with the grooved side up (flat side down).

4. Install the final drive sun gear (115) into the final drive carrier (116).