For 1990-2009 cars

Important:

• | Front wheel toe adjustment is performed with the steering wheel locked in the forward position.

• | Front toe is performed after rear toe and camber have been checked.

1. Position and lock the steering wheel with the vehicle with the wheels in the straight forward position.
2. Loosen both inner tie rod jam nuts.

Important: The inner tie rod must rotate freely from the boot seal surface. Do not allow the boot to rotate.

3. Loosen the inner tie rod seal to boot surface.
4. Use a wrench on the tie rod flats to increase or decrease the toe angle specifications. Refer to Wheel Alignment Specifications .

Notice: Refer to Fastener Notice in the Preface section.

5. Tighten the inner tie rod jam nuts.

Tighten
Tighten the jam nuts to 60 N·m (44 lb ft).

6. Inspect the toe angle to ensure proper adjustment and adjust as necessary.