For 1990-2009 cars

### Removal Procedure

1. Pull up on the control boot until the indicator bezel disengages from the console.
2. Disconnect the electrical connector from the indicator bezel.
3. Pull the boot up around the control knob to access the shift control indicator. Disengage the tabs on the indicator and remove.

### Installation Procedure

1. Install the shift control indicator into the indicator bezel.
2. Connect the indicator bezel electrical connector.
3. Install the indicator bezel into the console opening.