For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
ABS Sensor Bracket Bolt | 8 N·m | 71 lb in
Drive Axle Hub/Bearing Nut

- First Pass

115 N·m

85 lb ft

- Second Pass After Back Off

20 N·m

15 lb ft

- Final Pass

+ 90°

Lower Control Arm Ball Stud Pinch Bolt | 100 N·m | 74 lb ft
Lower Control Arm to Frame Bolts

- First Pass

90 N·m

66 lb ft

- Final Pass

+ 75° - 90°

Stabilizer Clamp Bolts | 20 N·m | 15 lb ft
Stabilizer Link Ball Stud Nuts | 65 N·m | 48 lb ft
Strut Shaft Nut | 55 N·m | 40 lb ft
Strut to Steering Knuckle Fasteners

- First Pass

50 N·m

37 lb ft

- Second Pass

100 N·m

73 lb ft

- Final Pass

+ 30° - 40°

Strut to Tower Nuts | 55 N·m | 40 lb ft
Tie Rod To Steering Knuckle Nut | 60 N·m | 45 lb ft