For 1990-2009 cars

### Removal Procedure

1. Remove the front bumper fascia. Refer to Front Bumper Fascia Replacement .
2. Remove the push-in retainers from the front energy absorber.
3. Remove the front energy absorber from the front bumper impact bar.

### Installation Procedure

1. Position the front energy absorber to the front bumper impact bar.
2. Install push-in retainers the energy absorber.
3. Install the front bumper fascia. Refer to Front Bumper Fascia Replacement .