For 1990-2009 cars

### Removal Procedure

1. Open the rear compartment.
2. Remove the nuts from the studs on the rear compartment lid applique.
3. Remove the rear compartment lid applique from the rear compartment lid.

### Installation Procedure

1. Position the rear compartment lid applique to the rear compartment lid.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the nuts to the studs on the rear compartment lid applique.

Tighten
Tighten the nuts to 5 N·m (43 lb in).

3. Close the rear compartment.