For 1990-2009 cars

Application | Specifications
--- | ---
Metric | English
A/C Compressor Clutch Coil Screws | 5 N·m | 44 lb in
A/C Compressor Clutch Plate Bolt | 12 N·m | 106 lb in
A/C Outlet to I/P Screws | 2.5 N·m | 22 lb in
A/C Refrigerant Pressure Sensor | 7 N·m | 62 lb in
Audio System Amplifier to I/P Beam Screws | 10 N·m | 89 lb in
Blower Motor Control Module | 3.0 N·m | 27 lb in
Blower Motor Housing Screws | 1.0 N·m | 9 lb in
Blower Motor Resistor Card Screws | 1.0 N·m | 9 lb in
Blower Motor Resistor Screws | 1 N·m | 9 lb in
Cluster Trim Plate to I/P Cluster Screws | 2.2 N·m | 22 lb in
Compressor Mounting Bolts (L61) | 22 N·m | 17 lb ft
Compressor Mounting Bolts (L81) | 20 N·m | 15 lb ft
Condensate Drain Tube Bolt | 3.5 N·m | 31 lb in
Condenser Block to Radiator End Tank Bolt | 5 N·m | 44 lb in
Condenser Hose Clamp to Condenser Screws | 6 N·m | 53 lb in
Condenser Hose to Condenser Block Bolt | 20 N·m | 15 lb ft
Condenser Hose to Condenser Block Fitting Bolt | 20 N·m | 15 lb ft
Condenser to Radiator Bolts | 5 N·m | 44 lb in
Console Fasteners | 2.5 N·m | 22 lb in
Control Head to I/P Screws | 2.5 N·m | 22 lb in
Discharge Hose Clamp to Cradle Screws | 5 N·m | 44 lb in
Discharge Hose to Compressor Bolt | 16 N·m | 12 lb ft
Discharge Hose to Condenser Block Bolt | 20 N·m | 15 lb ft
Evaporator Core Service Door to HVAC Module Screws | 1 N·m | 9 lb in
Evaporator Hose Assembly Clamp to Horn Bracket Nut | 10 N·m | 89 lb in
Evaporator Hose Assembly Clamps | 5 N·m | 44 lb in
Evaporator Hose Assembly to Condenser Hose Nut | 12 N·m | 106 lb in
Evaporator Hose Assembly to TXV Bolts | 7 N·m | 62 lb in
Evaporator Hose Assembly to Suction Pipe Nut | 12 N·m | 106 lb in
Fan Housing to Blower Motor Housing Screws | 1 N·m | 9 lb in
Filter Housing Screws | 3.5 N·m | 31 lb in
Filter Housing to HVAC Module Screws | 3.5 N·m | 31 lb in
Front of Dash Screen to Front of Dash Screws | 1 N·m | 9 lb in
HVAC Center Duct to HVAC Module Screws | 1 N·m | 9 lb in
HVAC Module Duct Screws | 1.0 N·m | 9 lb in
HVAC Module Screws | 1.0 N·m | 9 lb in
HVAC Module to Front of Dash Bolts | 4.5 N·m | 40 lb in
Heater Core Retaining Strap Screw | 1.0 N·m | 9 lb in
Heater Primary Lever Screws | 1.0 N·m | 9 lb in
Instrument Cluster to I/P Housing Screws | 2.3 N·m | 22 lb in
I/P Attachment Screws | 20 N·m | 15 lb ft
I/P Beam Inner Studs | 20 N·m | 15 lb ft
I/P Beam Outer Bolts | 7 N·m | 62 lb in
I/P Beam to Steering Column Brace Nuts | 20 N·m | 15 lb ft
I/P Bracket Nuts | 20 N·m | 15 lb ft
I/P Bracket to Floor Panel Nuts | 20 N·m | 15 lb ft
I/P Cluster Trim Plate to I/P Housing Fasteners | 2.5 N·m | 22 lb in
I/P to Radio Screws | 2.5 N·m | 22 lb in
Lower Fan Shroud Retaining Nuts | 5 N·m | 44 lb in
Mode Actuator Screws | 1.0 N·m | 9 lb in
Nut to Harness Clip | 6 N·m | 53 lb in
Pressure Relief Valve to Compressor | 12 N·m | 106 lb in
Radio to I/P Screws | 2.5 N·m | 22 lb in
Rear Shoulder Belt to C-Pillar | 35 N·m | 26 lb ft
Receiver Dehydrator Block Bolts | 3 N·m | 27 lb in
Receiver Dehydrator Clamp Bolt | 5 N·m | 44 lb in
Recirculation Actuator Bracket to HVAC Module Screws | 1.0 N·m | 9 lb in
Seat Attachment Nuts | 25 N·m | 19 lb ft
Shoulder Belt to Seat Frame Bolts | 35 N·m | 26 lb ft
Splash Shield Screws | 5 N·m | 44 lb in
Suction Pipe to Compressor Bolt | 16 N·m | 12 lb ft
TXV to Evaporator Core Block Bolts | 7 N·m | 62 lb in
Valve Assembly to Service Port Base | 12 N·m | 106 lb in
Vent Primary Lever Screws | 1.0 N·m | 9 lb in
Wiper Arm Assembly Nuts | 12 N·m | 106 lb in
Wiper Module Bolts | 5 N·m | 44 lb in