For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
Schematic Reference: Headlights/Daytime Running Lights (DRL) Schematics
1 | Did you perform the Lighting System Diagnostic System Check? | Go to Step 2 | Go to Diagnostic System Check - Lighting Systems
2 |

• | Turn ON the ignition switch, with the engine OFF.

• | Place the headlamp switch in the OFF position.

• | Ensure the parking brake is disengaged.

Does the DRL indicator illuminate?

Go to Testing for Intermittent Conditions and Poor Connections in Wiring Systems

Go to Step 3

3 | Are the daytime running lights illuminated? | Go to Step 4 | Go to Diagnostic System Check - Lighting Systems
4 | Replace the instrument cluster (IPC). Refer to Instrument Cluster Replacement . Did you complete the repair? | Go to Step 5 | --
5 | Operate the system in order to verify the repair. Did you correct the condition? | System OK | Go to Step 3