For 1990-2009 cars

### Removal Procedure

Notice: The throttle position (TP) sensor is an electrical component, and must NOT be soaked in any liquid solvent or damage may occur.

1. Turn the ignition OFF.
2. Disconnect the TP sensor harness connector.
3. Remove the TP sensor attachment screws and remove the TP sensor.

### Installation Procedure

1. Clean the O-ring sealing surface and the throttle shaft. Make sure the O-ring is seated in the TP sensor.
2. With the throttle plate closed, install the TP sensor over the throttle shaft.
3. Apply LOCTITE 242® Threadlocker to the threads of the TP sensor attachment screws and install the screws.

Tighten
Tighten the throttle position sensor screws to 2 N·m (18 lb in).

4. Connect the TP sensor harness connector. Push in the connector until a click is heard and pull back to confirm a positive engagement.