For 1990-2009 cars

#### Tools Required

J 44298 Driver Air Bag Removal Tool

Caution: Refer to SRS Sodium Hydroxide Powder Caution in the Preface section.

Caution: Refer to SIR Inflator Module Handling and Storage Caution in the Preface section.

Important: In the event deployment has occurred, refer to Repairs and Inspections Required After a Collision .

### Removal Procedure

Caution: Refer to SIR Caution in the Preface section.

1. Disable the SIR system. Refer to SIR Disabling and Enabling .
2. Remove the upper steering column trim cover. Refer to Steering Column Trim Covers Replacement .
3. Turn the steering wheel to the 3 o'clock position.
4. Adjust and install J 44298 into the 2 openings on the back side of the steering wheel.
5. Pull the handle toward the steering wheel. Release the 2 spring-loaded fasteners.
6. Turn the steering wheel. Repeat the same steps for the remaining 2 openings.
7. Disconnect the wiring and remove the bag.

### Installation Procedure

1. Connect the wiring to the air bag.
2. Align the air bag studs with holes in the steering wheel and press into position.

Important: Press each corner of the air bag until all spring retainers snap into position.

3. Install the upper steering column trim cover. Refer to Steering Column Trim Covers Replacement .
4. Enable the SIR system. Refer to SIR Disabling and Enabling .