For 1990-2009 cars

### Removal Procedure

Caution: When a hood hold open device is being removed or installed, provide alternate support to avoid the possibility of damage to the vehicle or personal injury.

1. Open and support the lift gate.
2. Lift up and partially remove the spring clips on the assist rods using a small flat-bladed tool.
3. Remove the upper end of the assist rods from the ball joint.
4. Remove the lower end of the assist rods from the ball joint.
5. Remove the assist rods from the lift gate.

### Installation Procedure

1. Position the assist rods to the lift gate.
2. Install the upper end of the assist rods to the ball joint. Press into place until fully seated.
3. Install the lower end of the assist rods to the ball joint. Press into place until fully seated.
4. Remove the support from the lift gate.
5. Close the lift gate.