For 1990-2009 cars

Important: The preferred method of dislodging the 2nd clutch piston is with compressed air. If compressed air is not available, remove the 2nd clutch piston assembly using pliers. If compressed air is used, note the following. Use a 9.5 mm (3/8 in) rubber hose on the air connection to reach into the 2nd clutch annulus port. When shooting air into the annulus port, ensure that the rubber hose covers both of the 2nd clutch annulus port holes.

1. Position the rubber hose so that the hose covers both 2nd clutch annulus holes (1).
2. Shoot air into the 2nd clutch annulus port until the 2nd clutch piston assembly (1) is dislodged.
3. Remove the 2nd clutch piston assembly (1).