For 1990-2009 cars

### Removal Procedure

1. Remove the windshield garnish molding. Refer to Windshield Garnish Molding Replacement in Interior Trim.
2. Partially pull down the headliner to expose the front drain hose. Refer to Headlining Trim Panel Replacement in Interior Trim.
3. Disconnect the front drain hose from the sunroof drain spouts.
4. Pull the front drain hose out from the inside of the vehicle.

### Installation Procedure

Important: Rotating the front drain hose while installing prevents the hose from kinking.

1. Route the front drain hose through the sunroof drain holes in the windshield pillar.
2. Connect the front drain hose to the sunroof drain spouts.
3. Reposition the headliner. Refer to Headlining Trim Panel Replacement in Interior Trim.
4. Install the windshield garnish molding. Refer to Windshield Garnish Molding Replacement in Interior Trim.