For 1990-2009 cars

### Removal Procedure

1. Remove the compartment fasteners.
2. Open the compartment door.
3. Remove the compartment door from the instrument panel (I/P).
4. Remove the compartment door fasteners. Separate the inner from the outer panel.
5. Remove the latch from the handle connector rod and remove the latch assembly.

### Installation Procedure

1. If the glove compartment door cover is being replaced, remove the spring clip and transfer the handle assembly to the new cover.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the latch with the latch fasteners.

Tighten
Tighten the latch fasteners to 2 N·m (18 lb in).

3. Install the connector rod.
4. Install the inner cover to the outer cover.

Tighten
Tighten the fasteners to 2 N·m (18 lb in).

5. Hold the hinge in the open position.
6. Guide the swing arm (1) into the opening. Close the compartment door.
7. Install the middle fastener.
8. Install the remaining 2 fasteners.
9. Verify the operation of the compartment door.