For 1990-2009 cars

#### Tools Required

J 38122-A Crankshaft Pulley Holder

1. Lubricate the front oil seal and seal surface of the crankshaft balancer with an engine oil supplement.

Notice: Misalignment of the keyway may cause damage to the oil pump.

2. Install the damper onto the crankshaft indexing keyway. Use care to properly align the keyway and flats on the damper with the oil pump drive.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the new retaining bolt and washer using the J 38122-A and a breaker bar to hold the crankshaft.

Tighten
Tighten the crankshaft pulley bolt to 100 N·m (74 lb ft) plus 75 degrees.