For 1990-2009 cars

#### Tools Required

• | 87 92 210 Differential Bearing Support

• | SA9120T Differential Bearing Installer

• | SA9172G Ball Detent Handle

### Assembly Procedure

1. Press the differential bearings onto the differential assembly using the SA9120T and the SA9172G . Use the 87 92 210 under the differential as shown.
2. To change the differential bearing races, refer to Clutch Housing Disassemble and Clutch Housing Assemble and Transmission Case Disassemble and Transmission Case Assemble