For 1990-2009 cars

### Removal Procedure

1. Remove the front seat from the vehicle. Refer to Front Seat Replacement - Bucket .
2. Remove the outer side trim from the seat cushion. Refer to Front Seat Front Finish Panel Replacement .
3. Disconnect the wiring harness from the motor on the power seat height adjuster.
4. Remove the screws from the height adjuster motor and remove the motor.

### Installation Procedure

1. Connect the wiring harness to the seat height adjuster motor.
2. Position the motor to the seat adjuster while pushing on the seat cushion to align the motor gears to the seat adjuster.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the seat motor screws.

Tighten
Tighten the screws to 2.5 N·m (22 lb in).

4. Install the outer side trim to the seat cushion. Refer to Front Seat Front Finish Panel Replacement
5. Install the front seat. Refer to Front Seat Replacement - Bucket .