For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel (I/P) cluster trim bezel. Refer to Instrument Panel Cluster Trim Plate Bezel Replacement .
2. Position the steering column to its lowest position.
3. Remove the cluster fasteners.
4. Remove the cluster from the I/P.

### Installation Procedure

1. Install the cluster into the I/P.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the fasteners.

Tighten
Tighten the fasteners to 2.5 N·m (22 lb in).

3. Install the I/P cluster trim bezel. Refer to Instrument Panel Cluster Trim Plate Bezel Replacement .