For 1990-2009 cars

### Removal Procedure

1. Insert a flat bladed tool between the cupholder and console.
2. Pry the cupholder assembly out.
3. Remove the cupholder from the console.

### Installation Procedure

1. If replacing the cupholder, transfer the inside lining to the new cupholder.
2. Install the cupholder to the console.
3. Press on the corners until the tabs are fully seated in the console.