For 1990-2009 cars

Important:

• | Measure as described below at a minimum of 3 locations.

• | Replace any 1-2-3-4 clutch steel plate that does not meet specifications.

1. Measure the thickness of each 1-2-3-4 clutch steel plate (1) at dimension A.

Specification
The 1-2-3-4 clutch steel plate minimum thickness is 2.135 mm (0.084 in).

Important: Check the plates for coning on a level surface.

2. Measure the cone of each plate (1) at dimension A.

Specification
The 1-2-3-4 clutch steel plate maximum cone is 0.200 mm (0.0079 in).