For 1990-2009 cars

### Removal Procedure

1. Remove the front seat. Refer to Front Seat Replacement - Bucket .
2. Remove the seat back pad/cover. Refer to Front Seat Back Cushion Cover and Cushion Pad Replacement .
3. Disconnect the electrical connections from the actuator motor to the seat back power recliner.
4. Remove the pal nut from the recliner actuator shaft.
5. Partially remove the shaft, then remove the recliner motor fasteners and the recliner actuator motor.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the recliner actuator motor and the fasteners.

Tighten
Tighten the fasteners to 6 N·m (53 lb in).

2. Install the actuator shaft to the seat back recliner and secure with the pal nut.
3. Connect the electrical connections to the actuator motor on the seat back power recliner.
4. Install the seat back pad and cover. Refer to Front Seat Back Cushion Cover and Cushion Pad Replacement .
5. Install the front seat. Refer to Front Seat Replacement - Bucket .