For 1990-2009 cars

### Removal Procedure

1. Remove the door trim panel. Refer to Front Side Door Trim Panel Replacement in Doors.
2. Remove the speaker fasteners and pull the speaker away from the door assembly.
3. Disconnect the wire harness from the speaker.
4. Remove the speaker from the vehicle.

### Installation Procedure

1. Connect the wire harness to the speaker.
2. Position the speaker in the door assembly, with the word TOP at the top of the speaker.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the fasteners.

Tighten
Tighten the fasteners to 1.5 N·m (13 lb in).

4. Install the door trim panel. Refer to Front Side Door Trim Panel Replacement in Doors.