For 1990-2009 cars

Illustration | Tool Number/ Description
--- | ---
| J 3555-92 Pressure Adapter For Mighty Vac
| J 7754-C Torque Wrench Beam Type
| J 25031-A Three Jaw Puller
| J 43482 Clutch Alignment Arbor
| J 43483 Impact Driver
| J 43628 Frame Alignment Fixture
| J 43707 Transaxle Support Fixture
| J 43915 Brake Bleeder Adapter
| J 43964 Engine Stand Fixture Adapter
| J 44015 Steering Linkage Installer
| J 44362 Input Shaft Support
| SA9105E Engine Support Fixture (3-Bar)
| SA9113T Axle Seal Installer
| SA9120T Differential Bearing Installer
| SA9133T Axle Seal Puller
| SA9172G Ball Detent Handle
| SA9179NE Dial Indicator
| SA9180NE Vacuum Pump
| SA9211T-2 5th Gear Remover
| SA9211T2-4 Thread On Adapter
| SA91100C Tie Rod Separator
| SA91112T Axle Seal Protector
| 78-41-067 Sleeve Inner Driver
| 83-90-114 Sleeve
| 83-90-312 Drift, Bearing Race Input Shaft
| 87-90-636 Pinion Fixture
| 87-90-800 Drift, Differential Seal
| 87-90-867 Input Shaft Bearing Ring
| 87-91-121 Input Shaft Bearing Puller Ring
| 87-91-188 Screw Press Support
| 87-91-204 Output Shaft Bearing Race Sleeve
| 87-91-220 Drift, Main Shift Rod Bushing
| 87-91-261 Output Shaft Remover
| 87-91-287 Puller
| 87-91-295 Puller Arms, 300 mm
| 87-91-311 Sleeve, Bearing Driver Shaft
| 87-91-410 Output Shaft Protector
| 87-91-428 Driver
| 87-91-642 Basic Puller
| 87-91-972 Assembly Ring
| 87-92-053 Companion Flange
| 87-92-061 Millimeter Disc
| 87-92-095 Weight 10 Kilogram
| 87-92-103 Output Shaft Assembly Tool
| 87-92-129 Lifting Eye
| 87-92-137 Milled Bearing Race
| 87-92-152 Input Shaft Bearing Puller
| 87-92-178 Output Shaft Puller Ring
| 87-92-202 Output Shaft Bearing Race Sleeve
| 87-92-210 Support, Differential Bearing
| 87-92-236 Support
| 87-92-335 Lock Pin Shift Linkage