For 1990-2009 cars

### Removal Procedure

Right front door shown. The rest of the doors are similar.

1. Insert a flat-bladed tool as shown in graphic.
2. Remove the lens.
3. Remove the bulb.
4. Remove the lamp housing and disconnect the wire connector.

### Installation Procedure

1. Install the wire connector.
2. Install the lamp housing.
3. Install the bulb.
4. Install the lens by pressing on the corners until the tabs are fully seated.