For 1990-2009 cars

The power seat adjuster motors are controlled through the power seat switch. Battery voltage is supplied to the power seat switch through the PWR SEATS 20A fuse. While the seat adjuster switches are in an inactive state the switch contacts are closed to the power seat switch ground circuit. When a power seat switch is pressed to an active state the switch contact is closed to the battery voltage supply circuit. Each seat adjuster motor is controlled by the power seat switch through 2 motor control circuits. The seat adjuster motors are bidirectional and the direction of adjuster motor rotation is determined by which of the adjuster motor control circuits is switched to battery voltage while the other remains grounded.