For 1990-2009 cars

1. Inspect the output shaft bushing (2) for wear or damage.
2. Measure the inside diameter (ID) of the bushing (2) at dimension A.
3. Replace the bushing If the ID of the bushing exceeds specifications.

Specification
The bushing maximum ID is 20.07 mm (0.794 in).

4. Measure the outside diameter (OD) of the bearing surface at dimension B.
5. Replace the output shaft if the OD of the bearing surface is less than specifications.

Specification
The bearing surface minimum OD is 44.978 mm (1.77 in).