For 1990-2009 cars

## Front Seat Front Finish Panel Replacement Inner

### Removal Procedure

1. Remove the front seat. Refer to Front Seat Replacement - Bucket .
2. Remove the screws from the inner recliner finish panel.
3. Remove the inner recliner finish panel.

### Installation Procedure

1. Install the inner recliner finish panel.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the screws to the inner recliner finish panel.

Tighten
Tighten the screws to 2.5 N·m (22 lb in).

3. Install the front seat. Refer to Front Seat Replacement - Bucket .

## Front Seat Front Finish Panel Replacement Outer

### Removal Procedure

1. Remove the front seat. Refer to Front Seat Replacement - Bucket .
2. In the case of manual seats, remove the recliner handle. Refer to Driver Seat and Passenger Seat Recliner Handle Replacement .
3. Remove the screws from the front seat finish panel.
4. Remove the front seat finish panel from the seat, starting at the recliner end of the panel.
5. In the case of power seats, disconnect the electrical connector from the switch.

### Installation Procedure

1. If you are installing a new finish panel, transfer the power seat switch to the new panel.
2. Install the front seat finish panel, starting at the front of the panel.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the screws to the finish panel.

Tighten
Tighten the screws to 2.5 N·m (22 lb in).

4. In the case of manual seats, install the recliner handle. Refer to Driver Seat and Passenger Seat Recliner Handle Replacement .
5. Install the front seat. Refer to Front Seat Replacement - Bucket .