For 1990-2009 cars

## Taillamps, Turn Signal, Stoplamps and Back-up Lamps Wagon

1. Open the liftgate.
2. Remove the interior access trim panel.
3. Rotate the bulb socket being replaced counter-clockwise 1/4 of a turn pressing the socket in firmly. Pull the socket rearward until the bulb clears the taillamp housing.
4. Replace it with the appropriate bulb.

## Taillamps, Turn Signal, Stoplamps and Back-up Lamps Sedan

1. Open the trunk.
2. Pull back the interior trim.
3. Remove the fasteners from the backside of the taillamp assembly.
4. Remove the taillamp assembly.
5. Rotate the bulb socket being replaced counter--clockwise 1/4 of a turn while pressing the socket in firmly. Pull the socket rearward until the bulb clears the taillamp housing.
6. Replace it with the appropriate bulb.