For 1990-2009 cars

### Removal Procedure

1. Remove the front door trim panel. Refer to Front Side Door Trim Panel Replacement .
2. Remove the front door water deflector. Refer to Front Side Door Water Deflector Replacement .
3. Remove the front door outer panel. Refer to Front Side Door Outer Panel Replacement .
4. Disconnect the electrical connectors.
5. Disconnect the wiring retainers from the door structure.
6. Remove the 2 rubber grommets.
7. Remove the wiring harness from the front door.

### Installation Procedure

1. Position the wiring harness to the front door.
2. Install the 2 rubber grommets.
3. Connect the wiring retainers to the door structure.
4. Connect the electrical connectors.
5. Install the front door outer panel. Refer to Front Side Door Outer Panel Replacement .
6. Install the front door water deflector. Refer to Front Side Door Water Deflector Replacement .
7. Install the front door trim panel. Refer to Front Side Door Trim Panel Replacement .