For 1990-2009 cars

### Removal Procedure

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection in Engine Electrical.
2. Remove the I/P compartment. Refer to Instrument Panel Compartment Replacement in Instrument Panel, Gages and Console.
3. Remove the right side heater duct assembly retainer.
4. Remove the right side heater duct assembly.
5. Disconnect the recirculation actuator electrical connector.
6. Remove the recirculation actuator bracket screws.
7. Remove the recirculation actuator assembly from the shaft.

Remove by pulling the assembly towards the front of the dash.

### Installation Procedure

1. Install the recirculation actuator assembly onto the door shaft.

The shaft has 2 flats that must be aligned to the actuator.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the recirculation actuator bracket to HVAC module screws.

Tighten
Tighten the screws to 1 N·m (9 lb in).

3. Connect the recirculation actuator electrical connector.
4. Install the right side heater duct assembly.
5. Install the right side heater duct assembly retainer.
6. Install the I/P compartment. Refer to Instrument Panel Compartment Replacement in Instrument Panel, Gages and Console.
7. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection in Engine Electrical.