For 1990-2009 cars

#### Tools Required

• | KM-671 Bushing Remover/Installer

• | KM-906-B Bushing Remover/Installer

### Removal Procedure

1. Remove the trailing arm from the vehicle. Refer to Trailing Arm Replacement .
2. Using the KM-671 and KM-906-B , assemble the KM-906-62, KM-906-61 and KM-671 arbor and press out the upper and lower control arm bushings.
3. Remove the M-906-62, KM-906-61, KM-671 arbor and bushing from the trailing arm.
4. Using the KM-671 and KM-906-B , assemble the KM-906-41, KM-906-44 and KM-671 arbor and press out the trailing arm front bushing.
5. Remove the KM-906-41, KM-906-44, KM-671 arbor and bushing from the trailing arm.

### Installation Procedure

1. Using the KM-671 and KM-906-B , assemble the KM-906-42, KM-906-43, KM-671 arbor and bushing to press in the trailing arm front bushing.
2. Remove the KM-906-42, KM-906-43, and KM-671 arbor from the trailing arm.
3. Using the KM-671 and KM-906-B , assemble the KM-906-63, KM-906-64 and KM-671 arbor and press in the upper and lower control arm bushings.
4. Remove the M-906-63, KM-906-64, and KM-671 arbor from the trailing arm.
5. Install the trailing arm to the vehicle. Refer to Trailing Arm Replacement .