For 1990-2009 cars

### Removal Procedure

1. Place a drain pan or suitable container under the vehicle.
2. Remove the upper transaxle cooler line from the radiator.
3. Raise the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
4. Remove the lower transaxle cooler line from the radiator.
5. Remove the transaxle oil cooler line assembly nut from the transaxle.
6. Remove the transaxle oil cooler line assembly from the vehicle.

### Installation Procedure

1. Install the transaxle oil cooler line assembly to the transaxle.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the transaxle oil cooler line assembly nut.

Tighten
Tighten the nut to 8 N·m (71 lb in).

3. Install the lower transaxle cooler line to the radiator.

Tighten
Tighten the fitting to 25 N·m (18 lb ft).

4. Lower the vehicle.
5. Install the upper transaxle cooler line to the radiator.

Tighten
Tighten the fitting to 25 N·m (18 lb ft).

6. Start the engine and inspect for leaks.
7. Inspect for proper fluid level. Refer to Transmission Fluid Check .