For 1990-2009 cars

### Removal Procedure

1. Remove the front door trim panel. Refer to Front Side Door Trim Panel Replacement .
2. Remove the front door water deflector. Refer to Front Side Door Water Deflector Replacement .
3. Remove the check link bolt at the hinge pillar.
4. Remove the check link nuts from the door frame.
5. Remove the check link from the door.

### Installation Procedure

1. Install the check link to the door frame.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the nuts to the check link.

Tighten
Tighten the nuts to 10 N·m (89 lb in).

3. Install the check link bolt.

Tighten
Tighten the bolt to 10 N·m (89 lb in).

4. Install the front door water deflector. Refer to Front Side Door Water Deflector Replacement .
5. Install the front door trim panel. Refer to Front Side Door Trim Panel Replacement .