For 1990-2009 cars

### Removal Procedure

1. Remove the front door window. Refer to Front Side Door Window Replacement .
2. Disconnect the electrical connection from the regulator, if equipped.
3. Remove the window regulator attachment bolts.
4. Remove the front door regulator out through the opening in the lower center door reinforcement.

### Installation Procedure

1. Install the front door regulator through the opening in the lower center door reinforcement.
2. Install and snug the regulator bolts, except the rear-most.
3. Leave the rear-most regulator attachment bolt out to allow for the window installation.
4. Install the front door window. Refer to Front Side Door Window Replacement .

Notice: Refer to Fastener Notice in the Preface section.

5. Install the regulator bolts.

Tighten
Tighten the bolts to 10 N·m (89 in lb).

6. Connect the electrical connector to the front door regulator, if equipped.
7. Inspect the front door regulator for proper operation. If binding exists, inspect all of the weatherstrips and adjust as necessary.
8. Install the front door water deflector. Refer to Front Side Door Water Deflector Replacement .
9. Install the front door inner panel. Refer to Front Side Door Trim Panel Replacement .