For 1990-2009 cars

### Removal Procedure

1. Disconnect the electrical connector from the for lamp.
2. Use a small flat-bladed tool to release the two fog lamp retainer tabs.
3. Remove the fog lamp from the fog lamp bezel.

### Installation Procedure

1. Position the fog lamp to the fog lamp bezel.
2. Install the fog lamp to the fog lamp bezel by pressing into place until fully seated.
3. Connect the electrical connector to the fog lamp.