For 1990-2009 cars

#### Tools Required

• | J 22912-01 Split Plate

• | J 23907 Slide Hammer

• | J 26941 Transmission Case Bearing Cup Remover

• | J 34757 Circlip Remover

• | J 35664 Bearing Installer

• | J 36850 Transjel® Transmission Assembly Lubricant

• | J 37209 Stub Shaft Seal Installer

• | J 37753 Bearing Installer

### Removal Procedure

1. Remove the input shaft needle bearing from the input shaft.
2. Use the J 34757 in order to remove the front input shaft bearing C-clip from the input shaft.
3. Use the J 22912-01 and a press arbor in order to remove the front input shaft bearing (2) from the input shaft (1).
4. Use the J 26941 and the J 23907 in order to remove the front input shaft oil seal (1) from the input shaft bearing retainer.
5. Clean the input shaft components with solvent. Air dry the components.
6. Clean the input shaft bearing retainer mating surface.
7. Inspect the shaft for scoring or excessive wear. Replace the shaft as necessary.
8. Inspect the shaft bearing for roughness or wear. Replace the shaft bearing as necessary.
9. Inspect the shaft needle bearing for roughness or damage. Replace the shaft needle bearing as necessary.

### Installation Procedure

1. Apply J 36850 to the input shaft bearing retainer seal surface.
2. Use a hammer and the J 37209 in order to install the new front input shaft oil seal (1) into the input shaft bearing retainer (2).
3. Use the J 37753 with the J 35664 and a press arbor in order to install the front input shaft bearing (1) onto the input shaft (2).
4. Install the front input shaft bearing C-clip (2) onto the input shaft.
5. Air-blow the lubrication oil hole (1) .
6. Apply J 36850 to the input shaft needle bearing.
7. Install the input shaft needle bearing (1) into the input shaft (2).