For 1990-2009 cars

#### Tools Required

• | J 36190 Universal Drive Handle

• | J 36511 Oil Plug Hex Bit

• | J 36798 Shift Rail Bushing Staking Tool

• | J 45379 Rear Seal Installer

1. Using the J 36190 (1) and the J 36798 (2), install the rear shift shaft bushing into the rear case.

• | Install the bushing on the J 36798-2 (2) with the collar end to hold the bushing.

• | Turn the J 36798-2 (3) over and stake the bushing with the stake end.

2. Install the shift shaft support and retaining ring into the rear case.

Important: Prior to installing the slip yoke oil seal, apply petroleum jelly between the lips of the seal.

3. Using the J 45379 , install the slip yoke oil seal into the rear case.
4. Apply pipe sealant GM P/N 12346004 (Canadian P/N 10953480) or equivalent, to the threads of the oil drain plug.

Notice: Refer to Fastener Notice in the Preface section.

5. Using the J 36511 , install the oil drain plug into the rear case.

Tighten
Tighten the oil drain plug to 30 N·m (22 lb ft).