For 1990-2009 cars

### Removal Procedure

1. Remove the lift gate trim panel. Refer to Liftgate Trim Panel Replacement .
2. Disconnect the electrical connectors from the lift gate latch.
3. Remove the bolts from the latch.
4. Disconnect the lift gate latch cable from the latch using a small flat-bladed tool.
5. Remove the latch from the lift gate.

### Installation Procedure

1. Connect the lift gate latch cable to the latch.
2. Install the latch to the lift gate.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the bolts to the latch.

Tighten
Tighten the bolts to 10 N·m (89 in lb).

4. Connect the electrical connectors to the lift gate latch.
5. Install the lift gate trim panel. Refer to Liftgate Trim Panel Replacement .