For 1990-2009 cars

### Removal Procedure

1. Remove the left transmission mount. Refer to Transmission Mount Replacement - Side
2. Disconnect the power steering lines from the side transmission mount bracket.
3. Remove the side transmission mount bracket to transmission bolts.
4. Remove the side transmission mount bracket from the transmission.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the side transmission mount bracket tot he transmission.

Tighten
Tighten the Transmission mount bracket bolts to 90 N·m (66 lb ft).

2. Connect the power steering lines from the side transmission mount bracket.

Tighten
Tighten the power steering lines to mount bolt to 10 N·m (89 lb in).

3. Install the left transmission mount. Refer to Transmission Mount Replacement - Side