For 1990-2009 cars

### Removal Procedure

1. Remove the rear seat cushion from the vehicle. Refer to Rear Seat Cushion Replacement in Seats.
2. Remove the fastener from the center seat belt buckle and remove the center seat belt assembly.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Position the center seat belt buckle with the locating tab facing downward in the position slot. Install the buckle fastener.

Tighten
Tighten the fastener to 35 N·m (26 lb ft).

2. Install the rear seat cushion to the vehicle. Refer to Rear Seat Cushion Replacement in Seats.