For 1990-2009 cars

### Removal Procedure

1. Open the rear compartment.
2. Disconnect the electrical connectors from the rear compartment latch.
3. Remove the bolts from the latch.
4. Disconnect the lock cylinder actuator cable from the latch.
5. Remove the latch from the rear compartment lid.

### Installation Procedure

1. Position the latch to the rear compartment lid.
2. Connect the lock cylinder actuator cable to the latch.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the bolts to the latch.

Tighten
Tighten the bolts to 10 N·m (89 lb in).

4. Connect the electrical connectors to the rear compartment latch.
5. Close the rear compartment.