For 1990-2009 cars

## Transmission General Specifications F Trim Solenoid

#### F Trim Solenoid Specifications

Sump Temperature | Resistance
--- | ---
Degrees C | Degrees F | Ohms
0 | 32 | 9.5
20 | 68 | 10.5
40 | 104 | 11.5

## Transmission General Specifications C, D, E Solenoids

#### C, D, and E On/Off Shift Solenoid Specifications

Sump Temperature | Resistance
--- | ---
Degrees C | Degrees F | Ohms
0 | 32 | 20.0
20 | 68 | 22.0
40 | 104 | 24.5

## Transmission General Specifications Wear Limits

#### Torque Converter Wear Limits

Part Measured | Specification
--- | ---
Metric | English
Torque Converter Pump Hub Minimum OD | 58.250 mm | 2.2933 in
Torque Converter Pump Hub Minimum Distance Between Flats | 51.816 mm | 2.0400 in
Torque Converter Cover Pilot, Minimum OD | 43.080 mm | 1.6960 in
Ground Sleeve, Maximum ID at Turbine Shaft Sealring Bore | 45.450 mm | 1.7894 in
Ground Sleeve, Maximum Spline Wear | No visible wear mm | No visible wear
Ground Sleeve Bushing, Maximum ID | 33.850 mm | 1.3326 in
Front Support Thrust Washer Thickness | 1.490 mm | 0.0590 in
Rotating Clutch Housing Bushing, Maximum ID | 78.170 mm | 3.0776 in
Rotating Clutch Housing Rotating Seal Bore, Maximum ID | 74.050 mm | 2.9154 in
C1 Friction Plates Maximum Cone | 0.255 mm | 0.0100 in
C1 Friction Plates Minimum Thickness | 2.375 mm | 0.0935 in
C1 Friction Plates Minimum Oil Groove Depth | 0.200 mm | 0.0079 in
C1 Steel Reaction Plate Maximum Cone | 0.200 mm | 0.0079 in
C1 Steel Reaction Plate Minimum Thickness | 2.135 mm | 0.0841 in
C1 Backplate Maximum Cone | 0.000 mm | 0.0000 in
C2 Friction Plates Maximum Cone | 0.225 mm | 0.0089 in
C2 Friction Plates Minimum Thickness | 2.375 mm | 0.0935 in
C2 Friction Plates Minimum Oil Groove Depth | 0.200 mm | 0.0079 in
C2 Steel Reaction Plate Maximum Cone | 0.240 mm | 0.0094 in
C2 Steel Reaction Plate Minimum Thickness | 2.135 mm | 0.0841 in
Turbine Shaft Bushing, Maximum ID | 20.150 mm | 0.7933 in
Turbine Shaft Thrust Washer | 2.590 mm | 0.102 in
C3/C4 Friction Plate Maximum Cone | 0.225 mm | 0.0089 in
C3/C4 Friction Plate Minimum Thickness | 2.375 mm | 0.0935 in
C3/C4 Friction Plate Minimum Oil Groove Depth | 0.200 mm | 0.0079 in
C3/C4 Steel Reaction Plate Maximum Cone | 0.400 mm | 0.0157 in
C3/C4 Steel Reaction Plate Minimum Thickness | 2.440 mm | 0.0961 in
C3/C4 Spring Plate Maximum Cone | 0.400 mm | 0.0157 in
C3/C4 Spring Plate Minimum Thickness | 3.110 mm | 0.1224 in
C3 Backplate Maximum Cone | 0.000 mm | 0.0000 in
C3 Backplate Minimum Thickness | 15.325 mm | 0.6033 in
Thrust Plate Inner Rim, Minimum Thickness | 3.000 mm | 0.1181 in
C4 Backplate Maximum Cone | 0.000 mm | 0.0000 in
C4 Backplate Minimum Thickness | 15.400 mm | 0.6063 in
C5 Friction Plate Maximum Cone | 0.225 mm | 0.0089 in
C5 Friction Plate Minimum Thickness | 2.375 mm | 0.0935 in
C5 Friction Plate Minimum Oil Groove Depth | 0.200 mm | 0.0079 in
C5 Steel Reaction Plate Maximum Cone | 0.295 mm | 0.0116 in
C5 Backplate Maximum Cone | 0.000 mm | 0.0000 in
C5 Backplate Minimum Thickness | 17.900 mm | 0.704 in
Main Housing Clutch Plate, Spline Wear (Notching) | 1.150 mm | 0.0450 in
P1 Ring Gear, Maximum Spline Wear (Notching) | 0.130 mm | 0.0051 in
P1 Carrier Assembly Bushing, Maximum ID | 50.690 mm | 1.9957 in
P1 Carrier Assembly Thrust Washers Thickness | 1.490 mm | 0.0590 in
P1 Carrier Assembly Pinion Maximum End Play | 1.010 mm | 0.0400 in
P2 Ring Gear, Maximum Spline Wear (Notching) | 0.130 mm | 0.0051 in
P2 Ring Gear Thrust Washer Thickness | 1.490 mm | 0.0590 in
P2 Carrier Assembly Pinion Maximum End Play | 1.010 mm | 0.0400 in
P2 Carrier Bushing, Maximum ID | 36.575 mm | 1.4400 in
P3 Ring Gear, Maximum Spline Wear (Notching) | 0.130 mm | 0.0051 in
P3 Carrier Assembly Pinion Maximum End Play | 1.010 mm | 0.0400 in
Main Shaft Pilot, Minimum OD (Turbine Shaft and Output Shaft) | 19.987 mm | 0.7869 in
Main Shaft Journal, Minimum OD (P2 Carrier Bushing) | 36.405 mm | 1.4333 in
Output Shaft Bushing (2WD and 4WD), Maximum ID | 20.150 mm | 0.7933 in
Output Shaft (2WD and 4WD), Minimum Bearing Surface OD | 44.978 mm | 1.7708 in
Parking Pawl Gear Wear | 0.000 mm | 0.0000 in
Output Yoke, Output Seal Surface, Minimum OD | 65.080 mm | 2.5622 in