For 1990-2009 cars

Application | Specifications
--- | ---
Metric | English
A/C Pressure Sensor | 7 N·m | 13 lb ft
Battery Terminal Bolts | 17 N·m | 13 lb ft
Crankshaft Position Sensor Bolt | 10 N·m | 89 lb in
EI Module Screws | 8 N·m | 71 lb in
Engine Coolant Temperature Sensor | 20 N·m | 15 lb ft
Engine Oil Pressure Switch | 10 N·m | 89 lb in
EVAP Purge Solenoid Bracket Bolt | 10 N·m | 89 lb in
HO2S-2 Harness Clip-to-Heat Shield Bolt | 4 N·m | 35 lb in
HO2S-2 Sensor-to-Exhaust Pipe | 45 N·m | 33 lb in
Ignition Coil Housing Bolts | 10 N·m | 89 lb in
Knock Sensor Bolt | 25 N·m | 18 lb ft
Output Speed Sensor (OSS) Stud | 12 N·m | 9 lb ft
Oxygen Sensor-to-Exhaust Manifold Pipe | 45 N·m | 33 lb ft
Spark Plugs | 20 N·m | 15 lb ft
Starter Solenoid Harness Nuts (Large) | 9 N·m | 80 lb in
Starter-to-Engine Bolts | 40 N·m | 30 lb ft
Throttle Cable Bracket Nuts | 5 N·m | 44 lb in