For 1990-2009 cars

### Removal Procedure

1. Remove the I/P storage compartment. Refer to Instrument Panel Compartment Replacement in Instrument Panel, Gages and Console.
2. Remove the insulator support from the I/P.
3. Remove the right side heater duct retainer.
4. Remove the right side heater duct.
5. Disconnect the electrical connector from the mode actuator.
6. Remove the mode actuator screws.
7. Remove the mode actuator.

### Installation Procedure

1. Install the mode actuator.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the mode actuator screws.

Tighten
Tighten the screws to 1 N·m (9 lb in).

3. Connect the electrical connector to the mode actuator.
4. Install the right side heater duct.
5. Install the right side heater duct retainer.
6. Install the insulator support to the I/P.
7. Install the I/P storage compartment. Refer to Instrument Panel Compartment Replacement in Instrument Panel, Gages and Console.